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	1. IDENTIFICATION OF CHEMICAL PRODUCTS AND INFORMATION ON THE MANUFACTURER AND / OR SUPPLIER

	Technical name
	
	[bookmark: _GoBack]Anti-slip treatment for floors made of porcelain stoneware, tiles, mosaics «GEKKON» ТМ «DipoxSi Systems»

	Brief recommendations for use
	
	Recommended for processing wetted tile surfaces in swimming pools and saunas, kitchens, showers and bathrooms, toilets, medical institutions, catering establishments, shopping and office centers. Surfaces can be processed both indoors and outdoors.

	Name of the organization
	
	Limited Liability Company "Anturazh" 

	Address
	
	141420, Russian Federation, Moscow region, Khimki, Skhodnya microdistrict, st. Nekrasova, house 2, building 77, floor 4, part of the room 23

	Emergency telephone number
	
	+7-499-394-02-60

	Fax
	
	Absent

	Е-mail
	
	anturazh.co@mail.ru
info@anturazh.msk.ru

	Web-site
	
	Absent 

	2. GHS HAZARD IDENTIFICATION

	Classification

Warning marking
	
	- chemical products causing skin corrosion/irritation, class 3
- chemical products causing serious eye damage/irritation, class 2B

	Signal word
	
	Warning

	Hazard symbols
	
	No symbol       

	H-phrases


P-phrases
	Н
	H316: Causes mild skin irritation.
H320: Causes eye irritation.

P264: Wash hands thoroughly after handling.
P305+P351+P338: IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.
P332+P313: If skin irritation occurs: Get medical attention.
P337+P313: If eye irritation persists: Get medical attention.


	3.  COMPOSITION / INFORMATION ON INGREDIENTS

		Component (INCI)
	Concentration (%)
	Number CAS
	Number EC

	Water
	98
	7732-18-5
	231-791-2

	Orthophosphoric acid
	2
	7664-38-2
	231-633-2




	4.  FIRST AID MEASURES

	In case of contact with eyes
	
	Rinse with plenty of running water with the eye slit wide open for 15 minutes. Remove contact lenses if you use them and if it is possible to do so without difficulty. Seek medical attention with the product label.

	When exposed to skin
	
	Rinse with running water. Seek medical attention if necessary.

	If swallowed
	
	Rinse mouth with water, drink plenty of fluids, take activated charcoal. Seek medical attention if necessary.

	Inhalation
	
	Fresh air, rest, warmth. Seek medical attention if necessary.

	Most important symptoms
Potential Hazardous Effects
	
	If inhaled: dizziness, headache, lethargy, sore throat, cough, difficulty breathing.
In case of contact with the eyes: redness, lacrimation.
When exposed to the skin: redness, dryness, itching.  
If swallowed: salivation, nausea, vomiting, abdominal pain, diarrhea.

	5.  FIRE FIGHTING MEASURES

	Flammability
	
	Non-flammable substance.

	Thermal degradation products
	
	No information.

	Fire and explosion safety
	
	Fire and explosion hazard indicators are not achieved.

	Extinguishing Methods
	
	According to the main source of ignition.

	Extinguishing Specificity
	
	The combustion process may involve the product packaging, the combustion of which is accompanied by the release of toxic substances. 
Firefighter's combat clothing (jacket and trousers with removable heat-insulating linings) complete with a firefighter's rescue belt, mittens or gloves, a fire helmet, and special protective footwear.

	6.  MEASURES IN CASE OF ACCIDENTAL RELEASE/LEAKAGE

	Individual precautions
	
	Isolate the danger zone within a radius of at least 50 m. Enter the accident zone in protective clothing and breathing apparatus. Remove bystanders. Observe fire safety measures. Do not smoke. Provide first aid to victims.

	Environmental precautions
	
	Maximum sealing of containers, communications and other equipment; periodic monitoring of the content of harmful substances in the air of the working area; cleaning the air of production facilities to established standards before discharging into the atmosphere. Do not allow products to enter water bodies, soil, sewage systems.

	Contamination and cleaning
	
	Eliminate the leak while observing safety precautions. Pump the contents into a serviceable container or into a drain container while observing the conditions for mixing liquids. In case of an intensive leak, enclose with an earthen embankment. Cover the spill site with sand, wash with plenty of water, embank and prevent the substance from getting into surface waters. Cut off the surface layer of soil with contamination, collect and remove for disposal while observing safety precautions. Cover the cut areas with a fresh layer of soil. Call in neutralization specialists.

	7.  HANDLING AND STORAGE

	Precautions and safe handling
	
	The premises must be equipped with general exchange and local supply and exhaust ventilation, ensuring clean air in the working area. 
When working with the product, do not drink, eat, or smoke. Wash your hands thoroughly after work. Observe personal hygiene rules.  

	Precautionary measures

Safe storage
	
	Avoid contact with eyes. Do not inhale. Do not swallow. Do not apply to wounds or mucous membranes.
The product is packaged in bottles, polypropylene canisters and placed in a cardboard box for transportation. 
The product is stored at a temperature of no lower than 5°C and no higher than plus 100°C in covered dry warehouses in the manufacturer's packaging. 
It is not allowed to store cleaning products under direct exposure to sunlight and near heating devices. 
The warranty period of the product is at least 24 months from the date of manufacture in unopened packaging of the manufacturer.

	8.  INDIVIDUAL PROTECTION MEANS

	Individual protection
Equipment
Control
	
	During production, the premises must be equipped with general exchange and supply and exhaust ventilation, ensuring clean air in the working area.

	Individual protection means
	
	When working, it is necessary to use personal protective equipment: filter respirators, rubber gloves, safety glasses, work clothes.

	Eye protection
	
	   [image: C:\Users\Home\Desktop\get - копия.jpg]

	Respiratory Protection
	
	


	Hand skin protection
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	Workwear
	
	  [image: ]

	Special tools
	
	Аbsent

	9.  PHYSICAL AND CHEMICAL PROPERTIES

		Specifications
	     Indicators

	Appearance 
	A colorless, slightly cloudy liquid

	Odor
	Odorless

	рН
	4.7-5.5

	Freezing point, °C
	Minus 1

	Initial boiling point, °C
	105




	10. STABILITY AND REACTIVITY

	Chemical stability
	
	The product is stable when handling, storage and transportation conditions are met.

	Solubility 
	
	Dissolves in water.

	11.  TOXICOLOGICAL INFORMATION

	Acute toxicity
	
	Acute toxicity indices of orthophosphoric acid: 
LD50(oral, rats) = 2600 mg/kg 
LD50(dermal, rabbits) > 2000 mg/kg 
CL50(inhalation, 4 h, rats) = 15384 mg/m3


	Respiratory or skin sensitization
	
	Sensitizing effect not established.

	Mutagenicity
	
	There is no data indicating that the product or any components present in an amount greater than 0.1% are mutagenic or genotoxic.

	Carcinogenicity
	
	None of the components of this product, present in amounts exceeding or equal to 0.1%, is classified by the IARC as a probable, possible or confirmed carcinogen for humans.

	Reproductive toxicity
	
	Does not have a negative effect on the reproductive function of the body.

	Specific target organ toxicity -
single exposure
	
	It is not classified as a specific target organ toxicant.

	Specific target organ toxicity -
repeated exposure
	
	It is not classified as a specific target organ toxicant.

	Aspiration hazard
	
	It is not classified as dangerous during aspiration.

	Chronic effects
	
	No information 

	12.  ENVIRONMENTAL INFORMATION

	Aquatic microorganisms
	
	Ecotoxicity indices of orthophosphoric acid: 
EC50 (daphnia, 48 h) > 100 mg/l 
IC50 (algae, 72 h) > 100 mg/l

	Persistence and degradability
	
	No information.

	Bioaccumulation potential
Soil mobility
	
	No information.
No information.

	Other adverse effects 
	
	No other adverse environmental impacts (eg ozone depletion, endocrine disruption, global warming potential) are expected from the product.

	13.  WASTE MANAGEMENT

	
	
	Production waste is neutralized in accordance with sanitary norms and rules approved in accordance with the established procedure.
Issues of recycling and disposal of waste products in the production process should be carried out on a contractual basis with a company licensed for waste disposal.

	14.  TRANSPORT INFORMATION

	14.1 Number UN
	
	Absent.

	14.2 Proper shipping and transport names
	
	Shipping Name 
Absent.

Transport Name:
Anti-slip treatment for floors made of porcelain stoneware, tiles, mosaics «GEKKON» ТМ «DipoxSi Systems»

	14.3 Types of transport risks
	
	

	International Civil Aviation Organization/ International Air Transport Association
(ICAO / IATA)
	
	Not applicable.

	Danger / Class / Division
	
	

	Environmental hazards
	
	

	Signs
	
	

	International Maritime Dangerous Goods Code (IMDG)code
	
	Not applicable.

	Danger / Class / Division
	
	

	Danger to the aquatic environment
	
	

	Signs
	
	

	The Intergovernmental Organisation for International Carriage by Rail(MKMPOG) /European agreement concerning the transport of dangerous goods (DOPOG)
	
	Not applicable.

		Danger / Class / Division

	Signs


Code
	
	

	14.4 Group packing
	
	Not assigned.

	14.5 Environmental risks
	
	Absent.

	14.6 Environmental risks with the app. II to the International Convention for the prevention of pollution from ships (MARPOL) 73/78 и code International Code for the Construction and Equipment of Ships, Carriers Dangerous Chemicals in Bulk (MRG)
	
	It does not concern.

	14.7 Special precautions
	
	Absent.

	15.  REGULATORY INFORMATION
HMIS
	[bookmark: _Hlk179299454]НEALTH	
		1




	FLAMMABILITY                      
		0




	PHYSICAL HAZARD              
		0




	PERSONAL PROTECTION 
		I








	

NFPA 
REACH
GHS
MDGC
ICAO/IATA

	Аpplication II MARPOL 73/78
RID
АDR


	16.  ADDITIONAL INFORMATION

	We believe that the information contained here is current as of the date of this Material Safety Data Sheet and is being offered in good faith. Since the use of this information and these opinions and the terms of use of the product are not under the control of LLC "Anturazh", it is the user's obligation to determine the conditions for the safe use of the product.

	Gathered information:
	
	LLC "Anturazh"

	Actual date:
	
	17.06.2025

	Disclaimer:
	
	The information provided in this Material Safety Data Sheet is based on data that is believed to be accurate at the date of preparation of this Material Safety Data Sheet. No liability is accepted for any damage or injury caused by abnormal use or due to non-compliance with recommended practices. The above information and the product are provided that the person receiving them must make their own determination as to the suitability of the product for their specific purpose and provided that they accept the risk of their use. In addition, no permission is granted or implied for the application of any patented invention without a license. The above information is believed to be accurate and reflect the information available to the manufacturer. However, this does not entail a guarantee for all the specific characteristics of the goods and does not serve as a basis for the emergence of contractual relations from a legal point of view. Current laws and regulations must be respected by the manufacturer’s successor  under his responsibility.

	
General director 
LLC "Anturazh"
                                                         
                                              / Tyunkov S.V. /

Print place
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